
==================================================
PL23XX Driver Setup Installer, Prolific Edition
Setup Installer Revision Note History
==================================================

System Requirement:
  . USB 1.1/2.0/3.0/3.1 Host Controller
  . Device using PL2303GC/GS/GT/GL/GE PL2323 version chips
  . Device using PL2303HXD/EA/RA/SA/TA/TB version chips
  . Supports the following Windows OS Family (32 and 64 bit):       
	- Windows 7 
	- Windows Server 2008R2 
	- Windows 8 
	- Windows Server 2012 
	- Windows 8.1
	- Windows Server 2012R2 
	- Windows 10 (TH1/TH2/RS1/RS2/RS3/RS4/RS5/19H1/19H2/20H1/20H2/21H1)
	- Windows Server 2016
	- Windows Server 2019
	- also compatible with POSReady and Windows Embedded Industry

	NOTE: 
	- Windows 98/ME/2000/XP driver technical support are discontinued.

 
Supported device ID and product strings:
  . VID_067B&PID_23A3 for "Prolific PL2303GC USB Serial COM Port" (PL2303G series)
  . VID_067B&PID_23C3 for "Prolific PL2303GT USB Serial COM Port" (PL2303G series)
  . VID_067B&PID_23D3 for "Prolific PL2303GL USB Serial COM Port" (PL2303G series)
  . VID_067B&PID_23E3 for "Prolific PL2303GE USB Serial COM Port" (PL2303G series)
  . VID_067B&PID_23F3 for "Prolific PL2303GS USB Serial COM Port" (PL2303G series)
  . VID_067B&PID_2323 for "Prolific PL2323 USB CDC Serial Port" (PL2303G series)
  . VID_067B&PID_2303 for "Prolific USB-to-Serial Comm Port" (PL2303 series)
  . VID_067B&PID_2304 for "Prolific USB-to-GPIO/PWM Port" (PL2303TB chip)

Driver Versions:
-------------------
	- PL2303G: WDF WHQL Driver: v5.1.0.0 (05/13/2021) - for Windows 7/8.1/10; Server2008/2008R2/2012/2012R2/2016/2019
	- PL2303:  WDF WHQL Driver: v3.8.39.0 (01/08/2021) - for Windows 7/8.1/10; Server2008/2008R2/2012/2012R2/2016/2019

Release Notes:
---------------
PL23XX Driver Installer v2.0.6
   Installer & Build date: 2.0.6 (2021-05-13)
	GUID:ECC3713C-08A4-40E3-95F1-7D0704F1CE5E
 
   =====================================================================
   PL2303G series Windows WDF WHQL Driver v5.1.0.0 (05/13/2021):
   =====================================================================
	Driver Revision Change:
	--------------------------------
        .  Modify BCD number.
        .  Fixed disable serial number issue on some Win7 USB 3.0 Host controller.

Previous History:
	Driver v5.0.17.0
	---------------------------------------------------
        .  Driver Certified for Windows 10 20H1  (version 2004)

	Driver v5.0.8.0
	---------------------------------------------------
        Driver Certified for Windows 10 19H1  (version 1903)

	Driver v5.0.7.15 (Driver Installer v1.3.0):
	---------------------------------------------------
        . Fixed EEPROM issue

	Driver v5.0.7.13 (Driver Installer v1.2.0):
	---------------------------------------------------
        . Driver Certified for Windows 10RS5  (version 1809)


   =====================================================================
   PL2303 series Windows WDF WHQL Driver v3.8.39.0 (01/08/2021):
   =====================================================================
	Driver Revision Change:
	--------------------------------
        .  PL2303TB: support RS485 mode.

Previous History:
	Driver v3.8.38.0 (12/01/2020)
	--------------------------------
        . Driver Certified for Windows 10 20H1  (version 2004)

	Driver v3.8.31.0 (07/30/2019)
	--------------------------------
        . Support special baud rate:3125000 bps

	Driver v3.8.30.0 (06/11/2019)
	--------------------------------
        . Driver Certified for Windows 10 19H1  (version 1903 build 18908)
	 

 

   Language Support: 
	- English (default)

Download Latest Driver here:
http://www.prolific.com.tw/US/ShowProduct.aspx?p_id=225&pcid=41


===========================
How to Install Driver
===========================
1. Unplug any PL23XX USB Device first.
2. Run Driver Installer EXE program to install. Wait to finish. 
3. Plug PL23XX USB Device and go to Device Manager to check COM Port number. 
4. If PL23XX is embedded, you might need to restart Windows or rescan hardware in Device Manager.
5. Refer to PL23XX Windows Driver User's Manual. 

NOTE: For silent install, include the syntax "/s" at the end of the EXE installer program. 
For example: "PL2303_Prolific_DriverInstaller_v1.10.0.exe /s"


===========================
How to do Silent Uninstallation
===========================
You need to create ISS response script to run silent uninstall or silent overwrite (update/modify). 

Example of how to create Uninstall script:
1. Copy your SETUP.EXE file to Temp folder.
2. Make sure you already run SETUP driver install beforehand. 
3. Run C:\TEMP\SETUP.EXE -r -f1¡¨C:\TEMP\uninstall.iss¡¨ and choose option Remove in dialog box. 
4. The file uninstall.iss will be created in Temp folder. 

To test silent uninstall:
1. Run ¡§C:\TEMP\SETUP.EXE -s¡¨ to install driver again.
2. Run C:\TEMP\SETUP.EXE -s ¡Vf1¡¨C:\TEMP\uninstall.iss¡¨ to silent uninstall.

=============================
How to do Silent Driver Update/Overwrite
==============================
Example of how to create Overwrite script:
1. Make sure you already run SETUP driver install beforehand. 
2. Run C:\TEMP\SETUP.EXE -r -f1¡¨C:\TEMP\overwrite.iss¡¨ and choose first option (Modify) in dialog box to install new driver (overwrite).

To test silent overwrite:
1. Run SETUP.EXE of old version. 
2. Run C:\TEMP\SETUP.EXE -s ¡Vf1¡¨C:\TEMP\overwrite.iss¡¨ to silent install new driver version. 

========================================
Prolific Technology Inc.
http://www.prolific.com.tw
